#### Back to index | # Info for nascom1

#### Nascom 1 & 2

Usage Notes:
The Nascom 2 clone has support for .cas, .bin and .nas cassette files.
The .cas files are used by BASIC. To get there from the monitor, type
EE000, enter 49152 as the memory size then CLOAD "<letter>". You can use

RUN/LIST etc. The <letter> for the existing cassettes are:
adventr.cas A
snailr.cas S
startrek.cas T
swinghs.cas M
swords.cas S
The .nas files are loaded by the monitor. Type L, wait for the loading to
finish, then E<start addr>. The start address is the address first
displayed by the load, usually 1000. To load the .bin files, use R in the
monitor.

created on Wed May 15 07:18:19 2002