#### Back to index | # Info for raaspec

#### RA+A Spectrum I+

Usage:
For the 8-button key mappings, see the user menu under "Keys (This Machine)".

This driver supports the LED backdrop images:
spec_bt.png
led.png

History and Trivia:
The Spectrum I+ was a modified Vectrex. It had a 32K ROM cart and 2K additional battery
backed RAM (0x8000 - 0x87ff). PB6 was used to signal inserted coins to the VIA. The
unit was controlled by 8 buttons (2x4 buttons of controller 1 and 2). Each button had a
LED which were mapped to 0xa000. The service mode can be accessed by pressing button 8
during startup. As soon as all LEDs light up, press 2 and 3 without releasing 8. Then
release 8 and after that 2 and 3. You can leave the screen where you enter ads by
pressing 8 several times.

created on Wed May 15 07:18:19 2002